(footprint "HF152FD_Form_A" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 62261D25)
  (attr through_hole)
  (fp_text reference "REF**" (at 6 -5.5 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 801b2c57-3824-49e5-89e3-7099dacfe6d1)
  )
  (fp_text value "HF152FD_Form_A" (at 6.4 -3.7 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 208846ef-9d16-4aea-8884-4ad489287be5)
  )
  (fp_line (start 17 13.9) (end 17 -2) (layer "F.SilkS") (width 0.12) (tstamp 049a0d59-31c4-4e8e-8965-d3040279d0ae))
  (fp_line (start 12.2 6.15) (end 12.2 10.85) (layer "F.SilkS") (width 0.12) (tstamp 20b31638-a6e0-490f-9160-2d6a76791db0))
  (fp_line (start -0.8 6) (end 8.1 6) (layer "F.SilkS") (width 0.12) (tstamp a577a535-624f-49ce-91f3-34c1213746d8))
  (fp_line (start 17 -2) (end -4.2 -2) (layer "F.SilkS") (width 0.12) (tstamp c1d01f2b-f45c-4cb9-b5bf-219aa60b0ea2))
  (fp_line (start -4.2 14) (end 17 14) (layer "F.SilkS") (width 0.12) (tstamp c8348631-404d-4e66-a92f-6abdda5d5496))
  (fp_line (start -4.2 -2) (end -4.2 14) (layer "F.SilkS") (width 0.12) (tstamp d169ccd3-ab8c-409f-8140-98ac4d80171c))
  (fp_line (start 13 3.75) (end 8.1 6) (layer "F.SilkS") (width 0.12) (tstamp fb9c178b-f3d0-4b11-be23-163bfb0daeef))
  (fp_rect (start -5.2 -3) (end 18 15) (layer "F.CrtYd") (width 0.05) (fill none) (tstamp 30abb9a4-6a70-4e36-840d-453db3cb840e))
  (pad "1" thru_hole circle (at 0 0) (size 2.3 2.3) (drill 1.3) (layers *.Cu *.Mask) (tstamp da302846-016d-4be2-af55-6d603d02eb89))
  (pad "2" thru_hole circle (at 0 12) (size 2.3 2.3) (drill 1.3) (layers *.Cu *.Mask) (tstamp c9b530ce-e490-420e-928e-df4bf9bc5adc))
  (pad "3" thru_hole circle (at -2 6) (size 2.3 2.3) (drill 1.3) (layers *.Cu *.Mask) (tstamp c164a52d-67af-4765-976d-f02114341851))
  (pad "4" thru_hole circle (at 12.2 12) (size 2.3 2.3) (drill 1.3) (layers *.Cu *.Mask) (tstamp c518c217-c92c-446b-ac12-3b43c18b8312))
)
