(footprint "CR2032_Holder" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 62261CA8)
  (descr "Coin Cell PV Battery Holder")
  (tags "CR2032")
  (attr through_hole)
  (fp_text reference "REF**" (at 7.3 -6.2 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 23c65112-425a-4ada-b1ca-3a5e5f538f08)
  )
  (fp_text value "CR2032_Battery_Holder" (at 7.3 -4.7 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 4ef94bb9-2e0a-4fb6-a2da-03965e6f684d)
  )
  (fp_text user "${REFERENCE}" (at 7.3 -3.2 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 65867e2e-3f24-4116-aeeb-b7c0d0114cc2)
  )
  (fp_line (start 2.54 -2.54) (end -1.7 -2.54) (layer "F.SilkS") (width 0.12) (tstamp 476b1128-2a06-4418-8c4e-6e9ca4d7e5b7))
  (fp_line (start 2.54 2.54) (end 2.54 -2.54) (layer "F.SilkS") (width 0.12) (tstamp 533854f6-ac37-46ef-b665-ba2d8aac1c93))
  (fp_line (start -1.7 2.54) (end 2.54 2.54) (layer "F.SilkS") (width 0.12) (tstamp b2600e4c-aec5-41d4-a697-836066376dce))
  (fp_circle (center -15.38 0) (end -1.5 0) (layer "F.SilkS") (width 0.12) (fill none) (tstamp 5b0557b9-b3ad-49ce-b3bc-d9e1ab30942e))
  (fp_line (start 3.4 3.4) (end 3.4 -3.4) (layer "F.CrtYd") (width 0.1) (tstamp 07d95c75-cc60-460d-8e32-ab4c50dd8b25))
  (fp_line (start -0.82 3.4) (end 3.4 3.4) (layer "F.CrtYd") (width 0.1) (tstamp 21b8ac40-eadf-4191-b4e4-7b4932f275a8))
  (fp_line (start 3.4 -3.4) (end -0.82 -3.4) (layer "F.CrtYd") (width 0.1) (tstamp 9add2b14-349f-4255-8bc9-6867c4ac3e1c))
  (fp_circle (center -15.38 0) (end -0.5 0) (layer "F.CrtYd") (width 0.1) (fill none) (tstamp 9e528cce-46ff-4bf2-83ab-a1ec37fb2e1f))
  (pad "1" thru_hole circle (at 0 0) (size 2 2) (drill oval 1.3 1.2) (layers *.Cu *.Mask) (tstamp 48d89f06-d1fb-4760-981e-831543f25182))
  (pad "2" thru_hole circle (at -20.49 0) (size 2 2) (drill 1.3) (layers *.Cu *.Mask) (tstamp 04216d84-e824-4bb3-b463-ea6199a58c8c))
)
