### outputs config
#

output eDP-1 pos 0 0
output DP-2 pos 1920 0
output DP-3 pos 1920 0
output DP-6 pos 3840 0

input 2:14:ETPS/2_Elantech_Touchpad {
	tap enabled
}

## inputs config

input 1386:827:Wacom_Intuos_S_2_Pen map_to_output eDP-1

input * {
	xkb_layout "fr"
	xkb_variant "azerty"
	xkb_options ""
	repeat_delay 300
	repeat_rate 60
}

input * xkb_numlock enable

### Function keys
#
	bindsym XF86AudioRaiseVolume exec pactl set-sink-volume @DEFAULT_SINK@ +5%
	bindsym XF86AudioLowerVolume exec pactl set-sink-volume @DEFAULT_SINK@ -5%
	bindsym XF86AudioMute exec pactl set-sink-mute @DEFAULT_SINK@ toggle
	bindsym XF86MonBrightnessDown exec brightnessctl set 5%- #TODO fix that
	bindsym XF86MonBrightnessUp exec brightnessctl set +5% #TODO fix that

	bindsym Ctrl+F12 output eDP-1 toggle

### Sreenshots
#
	# Take a screenshot with all output and save it into screenshots
	bindsym Print exec '$screenshot'

	# Take a screenshot of the select window
	bindsym Print+Ctrl exec '$screenshot_window'	

	# Take a Screenshot with the region select
	bindsym Print+Alt exec '$screenshot_select'
	
